**Breakbulk Americas 2021 - Exhibitor / Contractor Risk Assessment**

|  |  |  |
| --- | --- | --- |
| **Event:**  **Breakbulk Americas 2021** | **Venue:** | **Dates contractors in attendance on:**  **Move In:**  **Move out:** |
| **Exhibitors Details:**  **Name:**  **Address:**  **Phone:**  **Email:** | **Main Contractors Details:**  **Name:**  **Address:**  **Phone:**  **Email:** |
| **⬜ Please check this box to confirm you and your contractor(s) have fully read and understood the Breakbulk Americas COVID-19 exhibitor guidance**  **⬜ Please check this box to confirm you and your contractor(s) have fully read and understood the GRB Guidelines for Operating in Response to COVID-19**  **Both these documents can be found on the event website** [**here**](https://americas.breakbulk.com/page/exhibitor-manual) | | |
| **Risk Assessment undertaken by:** | **Risk Assessment accepted by:** | **Halls where working:** |
| **Signed:**  **Date:** | **Signed:**  **Date** | **Booth Number(s):** |
| **Subcontractor Company Names:** | | |

|  |
| --- |
| **Risk Profile: A brief description of the type of booth to be constructed, should include details such as, but not restricted to, the following:**  Is there any overhead rigging? Yes/No  Is this a double decker? Yes/No  Is this a complex\* booth/structure? Yes/No  Are there any complex\*\* lifts? Yes/No  Maximum expected attendance at any one time: |

\* A complex structure is any structure which requires structural calculations or includes any of the following:

* A multi-deck structure
* Is over 13ft (4m) in height
* Suspended loads over 400 kg
* Sound and lighting towers
* Tiered seating
* Stages and platforms for public use over 0.6m

\*\* Complex lifts are over 6.5ft (2m), or over 5,000 kg

| **Hazard** | **Risk**  **Level**  **L/M/H** | **Controls** | **Revised**  **Risk Level**  **L/M/H** |
| --- | --- | --- | --- |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |